Amanda Server Installation, backup and Recovry


Download latest version of amanda server package, installing the package.

#wget http://www.zmanda.com/downloads/community/Amanda/3.3.9/Redhat_Enterprise_6.0/amanda-backup_server-3.3.9-1.rhel6.x86_64.rpm

# rpm -ivh  amanda-backup_server-3.3.9-1.rhel6.x86_64.rpm

Enable amanda service in  xinetd:

#vim /etc/xinetd.d/amandaserver 

disable = no 
chkconfig xinetd on 

#service xinetd restart 
# su - amandabackup 
#mkdir /etc/amanda/DailyBackup 
#vim /etc/amanda/DailyBackup/amanda.conf 

org "DailyBackup"	# your organization name for reports 
mailto "amandabackup"	# space separated list of operators at your site 
dumpcycle 1 week	# the number of days in the normal dump cycle 
runspercycle 5          # the number of amdump runs in dumpcycle days 
			# (1 week * 5 amdump runs per week -- just weekdays) 
tapecycle 5 tapes	# the number of tapes in rotation 
			# 1 week (dumpcycle) times 5 tapes per week (just 
			# the weekdays) plus a few to handle errors that 
			# need amflush and so we do not overwrite the full 
			# backups performed at the beginning of the previous 
			# cycle 
runtapes 1		# number of tapes to be used in a single run of amdump 

define changer my_robot { 
tpchanger "chg-robot:/dev/sg10"
property "TAPE-DEVICE""0=tape:/dev/nst1""1=tape:/dev/nst0"
#    property append "tape-device""1=tape:/dev/nst1"
#    property append "tape-device""2=tape:/dev/nst0"
property "use-slots""1-30"
device-property "BLOCK_SIZE""512k"
} 

#tapedev "my_robot"
tpchanger "my_robot"
tapetype LTO5			# what kind of tape it is (see tapetypes below) 

holdingdisk hd2 { 
directory "/var/lib/amanda/holdings/DailyBackup"
use 1000 Mb 
} 

labelstr "^DailyBackup-[0-9][0-9]*$"	# label constraint regex: all tapes must match 

dtimeout 1800		# number of idle seconds before a dump is aborted. 
ctimeout 30		# maximum number of seconds that amcheck waits 
			# for each client host 
etimeout 300		# number of seconds per filesystem for estimates. 

define dumptype global { 
comment "Global definitions"
auth "bsdtcp"
} 

#define application-tool and dumptype for the amgtar application 
define application-tool app_amgtar { 
comment "amgtar"
plugin  "amgtar"
#property "GNUTAR-PATH""/path/to/gtar"
#property "GNUTAR-LISTDIR""/path/to/gnutar_list_dir"
} 

define dumptype gui-base { 
global 
program "APPLICATION"
application "app_amgtar"
comment "gui base dumptype dumped with tar"
compress none 
index yes 
} 

includefile "./advanced.conf"
includefile "/etc/amanda/template.d/dumptypes"
#includefile "/etc/amanda/template.d/tapetypes"

define tapetype LTO5 { 
comment "HP LTO5 FC - compression off"
length 1250000 mbytes 
filemark 0 kbytes 
speed 3000  kbytes           # 3.5 Mb/s 
} 



# su – amandabackup 
#mkdir /etc/amanda/DailyBackup/curinfo 
#mkdir /etc/amanda/DailyBackup/logs 
#mkdir /etc/amanda/DailyBackup/index
#touch /etc/amanda/DailyBackup/tapelist
#mkdir /var/lib/amanda/holdings/DailyBackup


#vim /etc/amanda/DailyBackup/changer.conf
havereader=1           #enables bracodes 
firstslot=1            #first slot for amanda to use 
lastslot=30            #last slot for amanda to use 
driveslot=0            #drive number  for amanda to use 
#for ((i=1; $i<=9;i++)); do amlabel  DailyBackup  DailyBackup-0$i slot $i;sleep 5;done
# vim /etc/amanda/DailyBackup/disklist
rsidcporcdb01   /RMANBACKUP/rsiprodbkp/BACKUP/BACKUP_23May16    global  -1

copy Amanda_client.tar.gz file into /tmp directory and run Amanda_client.sh, if script fails , kindly remove , amanda server information from /etc/hosts . (This script is for DC server , Kindly change hostname of DC amanda server  with DR server  hostname.)


Check config fine:
# amcheck DailyBackup

Run a Backup :

#amdump totalbackup

Recovery:

#amrecover 
>listhost (For Listing Host) 
>sethost HOSTNAME (FOR Setting Host) 
>listdisk    (For Listing Host) 
>setdisk DISKNAME (For Setting Disk) 
>history (For Listing History) 
>setdate 2013-03-26-17-38-09 (For Setting backup date) 
>ls (For Listing Files) 
>extract (For Extracting Backup)
